**GLEN A. TABOCLAON**

**POSITION DESIRED: Overhead Crane Operator**

**Launching Girder Operator/Lifting Frame**

**Operator/ Gantry Crane Operator/**

**PERSONAL DATA**

Age : 42

Sex : Male

Civil Status : Married

Height : 5”6’

Religion : Roman Catholic

Contact No. : 09668770892

Address : Purok #26 Poblacion, Manticao, Misamis Oriental

Philippines

Email Add. : glentaboclaon7@gmail.com

**EDUCATIONAL BACKGROUND**

Elementary : Manticao Central School (1991-1992)

High School : Saint Anthony High School (1995-1996)

College : Liceo de Cagayan University (under graduate)

**WORK EXPERIENCE**

**Bouygues Travaux Philippines**

(Launching Girder Operator)

September 7, 2020 to March 12, 2022

Makati Ctiy, Metro Manila

**Dragages Hong Kong Limited**

(Lifting Frame /Launching Gantry Operator)

November 11, 2015 to September 15, 2017

Hongkong

**Leighton Construction Company**

(Gantry Crane Operator)

February 4, 2010 to October 19, 2015

Brgy. 64 hizon PNR compound

Caloocan City, Manila

**Emirates Steel Industries**

(Overhead Crane Operator)

November 5, 2007- October 2009

Abu Dhabi, United Arab Emirates

**Saudi Iron and Steel Company (Hadeed-Sabic)**

(Overhead Crane Operator)

November 17, 2005-October 2, 2007

Jubail, Kingdom of Saudi Arabia

**Philippine Minerals and Alloy Corp.**

(Tower Crane Operator)

December 1999- December 2004

Manticao, Misamis Oriental, Philippines

**JOB DETAILS OF LAUNCHING GIRDER:**

* Deal, main hoist 1200 tons, auxiliary 5 tons.
* Main girder 2 box height 2290mm, weight 1380mm, length 52720mm, generator platform 3435mm.
* Support beam 1 mast, weight 2500mm, height 2175mm, length 54958mm.
* Overall dimensions, in 34m span configuration length 105630mm, weight 14000mm, height 10300mm.
* From the deck, height 8045mm from pier head.

**DUTIES AND RESPONSIBILITIES OF LAUNCHING GIRDER OPERATOR**

* Assembling of launching gantry (29m and 34m span).
* Stressing, stitching and epoxy application.
* Post tensioning of tendons and grouting of bearing plinths.
* I operate launching girder for erection of full span girders and segmental.

**JOB DETAILS:**

* Overhead Crane (KHOTEN) 10 tons auxiliary 75 tons man hoist, with cab and switch operation.
* Overhead Crane (DANIELI) 10 tons auxiliary and 25 tons man hoist, with cab and can switch operation.

**DUTIES AND RESPONSIBILITIES**

* Testing of overhead Crane during first hour of work for any abnormalities and report to maintenance for proper check-up.
* Daily check-up of electrical system/ equipment associated by duty electrician.
* Cleaning/ servicing of overhead crane as per schedule associated by duty electrician.
* Lifting of ladle, preparation during furnace tapping
* Segregation of slag to metal.
* Pouring metal to cooling molds, transport to sizing area.
* Assist slag tender, lifting of slag from slag runner transport to slag pit.
* Assist lifting of heavy equipment from ground floor to furnace lobby.
* To perform the duty smooth and orderly from time to time.

**DUTIES AND RESPONSIBILITIES OF GANTRY CRANE OPERATOR**

* Operate crane under general supervision.
* Manipulate or depress cane controls to regulate speed and direction of crane and hoist movement according to written, verbal, or signal instructions.
* Repair crane as needed.
* Inspect crane for safety issues on a daily basis.
* Determine if any parts are malfunctioning.
* Complete job tickets, service quality summaries, and all other necessary paperwork.
* Lift, position and place machinery, equipment or other large objects at construction sites and industrial facilities.
* Drive trucks to worksites and unload trucks.
* Place blocks and outriggers to prevent capsizing when lifting heavy loads.
* Move levers and pedals to rotate crane on chassis to raise and lower crane boom and to raise and lower load-line.
* Bolt boom sections together to extend or modify boom for pile driving or high lifting.
* Work with in precise limits and standards of accuracy.
* Operate crane according to signals from helper.
* Start and stop crane engine.
* Follow directions carefully.